**Floating Ark Directions:**

1. Prepare the “sea” by making waves on the construction paper with markers and decorating and applying little sticky tape fish. This piece should be laminated before proceeding to prevent water damage.

2. Attach the “sea” to the Styrofoam float using clear tape.

3. Close the Styrofoam float using clear tape.

Close the corrugated paper strip to create an oval for the body of the ark. Secure with tape on the inside of the oval, and position and tape the ark to the center of the “sea.”

4. Draw a little Noah, from the waist up, on the small white rectangle using markers and crayons. Cut it out and tape it to the bow or stern of the ark on the inside edge so that Noah is “looking out.”

5. Score the railroad board and the ark on the inside edge so that Noah is “looking out.”

Score the railroad board and ore the railroad board and fold along scored edge to form a peaked roof. This may be taped to the body of the ark or left as is so that it’s removable and little animals (another project!) can be stored in the ark.

\_\_